|  |  |
| --- | --- |
|

|  |
| --- |
| DFA-CA Specification  |

 |
|  |
| **TYPICAL SPECIFICATIONS** |
| **Model:**  | **DFA-CA**  |
|  |  |
| **Description:**  | Fan shall be galvanized, duct mounted, centrifugal, direct drive, exhaust fan.  |
|  |  |
| **Certifications:**  | Fan shall be listed to UL507 Standards.  |
|  |  |

|  |
| --- |
| **Construction:** **Housing**The fan housing shall be constructed of 20 gauge galvanized steel. The fan housing shall include an inlet and outlet duct connection, both made from stamped steel. A junction box of polymeric construction shall be mounted on the outer perimeter of the fan housing for ease of installation. The fan may be installed in ceiling, connected to ductwork.**Wheel**The fan wheel shall be polymeric or steel construction, centrifugal, and dynamically balanced for quiet, efficient performance. The wheel shall be firmly attached to the motor shaft with set screws.**Motor**Standard 115 volt, open drip motors shall be permanently lubricated, rated for continuous duty and thermally protected.**Product: Fan shall be model DFA-CA as manufactured by CaptiveAire Systems.** |